This is Matlab code for converting Geodetic coordinates to Cartesian coordinates and vice versa using the direct and indirect approaches.